EzyFit Function Reference | << Prev | Next >>

myginput
Graphical input from mouse with custum cursor pointer.
Description `

    [X,Y] = myginput(N) gets N points from the current axes and returns
    the X- and Y-coordinates in length N vectors X and Y.

    [X,Y] = myginput(N, POINTER) also specifies the cursor pointer, e.g.
    'crosshair', 'arrow', 'circle' etc. See "Specifying the Figure Pointer"
    in Matlab's documentation  to see the list of available pointers.

    myginput is strictly equivalent to Matlab's original GINPUT, except
    that a second argument specifies the cursor pointer instead of the
    default 'fullcrosshair' pointer.

Example

      plot(1:2,1:2,'s');
      hold on
      [x,y] = myginput(1,'crosshair');
      plot(x,y,'o');
      hold off

    myginput is copied from Matlab's GINPUT rev. 5.32.4.4.

See Also

    GINPUT.

`

Previous: makevarfit | Next: pickdata

2005-2008 EzyFit Toolbox 2.20